BR2_arm=y
BR2_cortex_a7=y
BR2_ARM_EABIHF=y
BR2_ARM_FPU_NEON_VFPV4=y

BR2_TOOLCHAIN_BUILDROOT_CXX=y

BR2_SYSTEM_DHCP="eth0"

# Linux headers same as kernel, a 4.4 series
BR2_PACKAGE_HOST_LINUX_HEADERS_CUSTOM_4_4=y

BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_GIT=y
BR2_LINUX_KERNEL_CUSTOM_REPO_URL="https://github.com/raspberrypi/linux.git"
BR2_LINUX_KERNEL_CUSTOM_REPO_VERSION="1ebe8d4a4c96cd6a90805c74233a468854960f67"
BR2_LINUX_KERNEL_DEFCONFIG="bcm2709"

# Build the DTB from the kernel sources
BR2_LINUX_KERNEL_DTS_SUPPORT=y
BR2_LINUX_KERNEL_INTREE_DTS_NAME="bcm2709-rpi-2-b"

BR2_PACKAGE_RPI_FIRMWARE=y
# BR2_PACKAGE_RPI_FIRMWARE_INSTALL_DTB_OVERLAYS is not set

# Required tools to create the SD image
BR2_PACKAGE_HOST_DOSFSTOOLS=y
BR2_PACKAGE_HOST_GENIMAGE=y
BR2_PACKAGE_HOST_MTOOLS=y

# Filesystem / image
BR2_TARGET_ROOTFS_EXT2=y
BR2_TARGET_ROOTFS_EXT2_4=y
# BR2_TARGET_ROOTFS_TAR is not set
BR2_ROOTFS_POST_BUILD_SCRIPT="board/raspberrypi2/post-build.sh"
BR2_ROOTFS_POST_IMAGE_SCRIPT="board/raspberrypi2/post-image.sh"
