From 59cce7b304a8cbbb508ba21ab2f9052d3ee9a9e3 Mon Sep 17 00:00:00 2001
From: Max Filippov <jcmvbkbc@gmail.com>
Date: Tue, 29 Nov 2016 13:09:17 -0800
Subject: [PATCH 2/2] xtensa: Fix PR target/78603

2016-11-29  Max Filippov  <jcmvbkbc@gmail.com>
gcc/
	* config/xtensa/xtensa.c (hwloop_optimize): Don't emit zero
	overhead loop start between a call and its CALL_ARG_LOCATION
	note.

Signed-off-by: Max Filippov <jcmvbkbc@gmail.com>
---
Backported from: r242979

 gcc/config/xtensa/xtensa.c | 5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

diff --git a/gcc/config/xtensa/xtensa.c b/gcc/config/xtensa/xtensa.c
index e49f784..70f698a 100644
--- a/gcc/config/xtensa/xtensa.c
+++ b/gcc/config/xtensa/xtensa.c
@@ -4158,7 +4158,10 @@ hwloop_optimize (hwloop_info loop)
       entry_after = BB_END (entry_bb);
       while (DEBUG_INSN_P (entry_after)
              || (NOTE_P (entry_after)
-                 && NOTE_KIND (entry_after) != NOTE_INSN_BASIC_BLOCK))
+                 && NOTE_KIND (entry_after) != NOTE_INSN_BASIC_BLOCK
+		 /* Make sure we don't split a call and its corresponding
+		    CALL_ARG_LOCATION note.  */
+                 && NOTE_KIND (entry_after) != NOTE_INSN_CALL_ARG_LOCATION))
         entry_after = PREV_INSN (entry_after);
 
       emit_insn_after (seq, entry_after);
-- 
2.1.4

