BR2_arm=y
BR2_cortex_a7=y
BR2_ARM_EABIHF=y
# Linux headers same as kernel, a 4.1 series
BR2_PACKAGE_HOST_LINUX_HEADERS_CUSTOM_4_1=y
BR2_TARGET_GENERIC_HOSTNAME="a20-olinuxino"
BR2_TARGET_GENERIC_ISSUE="Welcome to OLinuXino!"
BR2_TARGET_GENERIC_GETTY_PORT="ttyS0"
BR2_ROOTFS_POST_BUILD_SCRIPT="board/olimex/a20_olinuxino/post-build.sh"
BR2_ROOTFS_POST_IMAGE_SCRIPT="board/olimex/a20_olinuxino/post-image.sh"
BR2_ROOTFS_POST_SCRIPT_ARGS="board/olimex/a20_olinuxino/boot.cmd $(TARGET_DIR)/boot"
BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_VERSION=y
BR2_LINUX_KERNEL_CUSTOM_VERSION_VALUE="4.1.4"
BR2_LINUX_KERNEL_DEFCONFIG="sunxi"
BR2_LINUX_KERNEL_DTS_SUPPORT=y
BR2_LINUX_KERNEL_INTREE_DTS_NAME="sun7i-a20-olinuxino-lime2"
BR2_LINUX_KERNEL_INSTALL_TARGET=y
BR2_PACKAGE_SUNXI_TOOLS=y
BR2_PACKAGE_SUNXI_BOARDS=y
BR2_PACKAGE_SUNXI_BOARDS_FEX_FILE="a20/a20-olinuxino_lime.fex"
BR2_TARGET_ROOTFS_EXT2=y
BR2_TARGET_ROOTFS_EXT2_4=y
# BR2_TARGET_ROOTFS_TAR is not set
BR2_TARGET_UBOOT=y
BR2_TARGET_UBOOT_BUILD_SYSTEM_KCONFIG=y
BR2_TARGET_UBOOT_CUSTOM_VERSION=y
BR2_TARGET_UBOOT_CUSTOM_VERSION_VALUE="2016.05"
BR2_TARGET_UBOOT_BOARD_DEFCONFIG="A20-OLinuXino-Lime2"
BR2_TARGET_UBOOT_NEEDS_DTC=y
BR2_TARGET_UBOOT_SPL=y
BR2_TARGET_UBOOT_SPL_NAME="u-boot-sunxi-with-spl.bin"
BR2_PACKAGE_HOST_GENIMAGE=y
BR2_PACKAGE_HOST_UBOOT_TOOLS=y
