config BR2_PACKAGE_HOST_RASPBERRYPI_USBBOOT
	bool "host raspberrypi-usbboot"
	depends on BR2_arm
	help
	  This package builds and install the "rpiboot" tool for the
	  host machine. This tool allows to boot the Broadcom BCM
	  processor used in the RaspberryPi to boot over USB, and have
	  it expose a USB mass storage device in order to reflash the
	  built-in storage of the RaspberryPi (useful for the eMMC
	  built into the Compute module).

	  https://github.com/raspberrypi/usbboot
