BR2_arm=y
BR2_cortex_a7=y
BR2_ARM_FPU_VFPV4=y

# Cannot use same headers as the kernel, because kernel is 4.9
# and we only know 4.8 at best so far
BR2_KERNEL_HEADERS_4_8=y

BR2_TARGET_GENERIC_HOSTNAME="nanopi-neo"
BR2_TARGET_GENERIC_ISSUE="Welcome to Buildroot for the NanoPi NEO"
BR2_ROOTFS_POST_BUILD_SCRIPT="board/nanopi-neo/post-build.sh"
BR2_ROOTFS_POST_IMAGE_SCRIPT="board/nanopi-neo/post-image.sh"

# Use a -rc kernel to get the DTS
BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_VERSION=y
BR2_LINUX_KERNEL_CUSTOM_VERSION_VALUE="4.9-rc3"
BR2_LINUX_KERNEL_DEFCONFIG="sunxi"
BR2_LINUX_KERNEL_DTS_SUPPORT=y
BR2_LINUX_KERNEL_INTREE_DTS_NAME="sun8i-h3-nanopi-neo"

# Use an -rc tag because the defconfig is very recent
BR2_TARGET_UBOOT=y
BR2_TARGET_UBOOT_BUILD_SYSTEM_KCONFIG=y
BR2_TARGET_UBOOT_CUSTOM_VERSION=y
BR2_TARGET_UBOOT_CUSTOM_VERSION_VALUE="2016.11-rc3"
BR2_TARGET_UBOOT_BOARD_DEFCONFIG="nanopi_neo"
BR2_TARGET_UBOOT_NEEDS_DTC=y
BR2_TARGET_UBOOT_FORMAT_CUSTOM=y
BR2_TARGET_UBOOT_FORMAT_CUSTOM_NAME="u-boot-sunxi-with-spl.bin"

# Build an sdcard image
BR2_TARGET_ROOTFS_EXT2=y
BR2_TARGET_ROOTFS_EXT2_4=y
BR2_TARGET_ROOTFS_EXT2_BLOCKS=32768
BR2_TARGET_ROOTFS_EXT2_INODES=8192
# BR2_TARGET_ROOTFS_TAR is not set
BR2_PACKAGE_HOST_DOSFSTOOLS=y
BR2_PACKAGE_HOST_GENIMAGE=y
BR2_PACKAGE_HOST_MTOOLS=y
BR2_PACKAGE_HOST_UBOOT_TOOLS=y
